- **ASSINGMENT NO 5**

**Graphical user interface, text, application

Description automatically generatedQUESTION NO 1-**

**Text, application

Description automatically generated**

UART\_HandleTypeDef huart1;

/\* USER CODE BEGIN PV \*/

uint8\_t msg[] = "Hi, Welcome to UART demo!!\r\n";

uint8\_t msg1[] = "LED ON\r\n";

uint8\_t msg2[] = "LED Off\r\n";

uint8\_t rcv[12] = {0};

/\* USER CODE END PV \*/

/\* Private function prototypes -----------------------------------------------\*/

**void** **SystemClock\_Config**(**void**);

**static** **void** **MX\_GPIO\_Init**(**void**);

**static** **void** **MX\_USART1\_UART\_Init**(**void**);

/\* USER CODE BEGIN PFP \*/

/\* USER CODE END PFP \*/

/\* Private user code ---------------------------------------------------------\*/

/\* USER CODE BEGIN 0 \*/

/\* USER CODE END 0 \*/

/\*\*

\* @brief The application entry point.

\* @retval int

\*/

**int** **main**(**void**)

{

/\* USER CODE BEGIN 1 \*/

/\* USER CODE END 1 \*/

/\* MCU Configuration--------------------------------------------------------\*/

/\* Reset of all peripherals, Initializes the Flash interface and the Systick. \*/

HAL\_Init();

/\* USER CODE BEGIN Init \*/

/\* USER CODE END Init \*/

/\* Configure the system clock \*/

SystemClock\_Config();

/\* USER CODE BEGIN SysInit \*/

/\* USER CODE END SysInit \*/

/\* Initialize all configured peripherals \*/

MX\_GPIO\_Init();

MX\_USART1\_UART\_Init();

/\* USER CODE BEGIN 2 \*/

/\* USER CODE END 2 \*/

HAL\_UART\_Transmit(&huart1, msg, **sizeof**(msg), 100000);

HAL\_UART\_Receive(&huart1,rcv,10,100000);

HAL\_UART\_Transmit(&huart1, rcv, **sizeof**(msg), 100000);

/\* Infinite loop \*/

/\* USER CODE BEGIN WHILE \*/

**while** (1)

{

/\* USER CODE END WHILE \*/

/\* USER CODE BEGIN 3 \*/

**if**(\*rcv=='1')

HAL\_GPIO\_WritePin(led1\_GPIO\_Port, led1\_Pin, 1);

HAL\_UART\_Transmit(&huart1, msg1, **sizeof**(msg1), 1000);

HAL\_Delay(1000);

HAL\_GPIO\_WritePin(led1\_GPIO\_Port, led1\_Pin, 0);

HAL\_UART\_Transmit(&huart1, msg2, **sizeof**(msg2), 1000);

HAL\_Delay(1000);

}

/\* USER CODE END 3 \*/

}

/\*\*

\* @brief System Clock Configuration

\* @retval None

\*/

**void** **SystemClock\_Config**(**void**)

{

RCC\_OscInitTypeDef RCC\_OscInitStruct = {0};

RCC\_ClkInitTypeDef RCC\_ClkInitStruct = {0};

/\*\* Configure the main internal regulator output voltage

\*/

**if** (HAL\_PWREx\_ControlVoltageScaling(PWR\_REGULATOR\_VOLTAGE\_SCALE1) != *HAL\_OK*)

{

Error\_Handler();

}

/\*\* Initializes the RCC Oscillators according to the specified parameters

\* in the RCC\_OscInitTypeDef structure.

\*/

RCC\_OscInitStruct.OscillatorType = RCC\_OSCILLATORTYPE\_MSI;

RCC\_OscInitStruct.MSIState = RCC\_MSI\_ON;

RCC\_OscInitStruct.MSICalibrationValue = 0;

RCC\_OscInitStruct.MSIClockRange = RCC\_MSIRANGE\_6;

RCC\_OscInitStruct.PLL.PLLState = RCC\_PLL\_ON;

RCC\_OscInitStruct.PLL.PLLSource = RCC\_PLLSOURCE\_MSI;

RCC\_OscInitStruct.PLL.PLLM = 1;

RCC\_OscInitStruct.PLL.PLLN = 40;

RCC\_OscInitStruct.PLL.PLLP = RCC\_PLLP\_DIV7;

RCC\_OscInitStruct.PLL.PLLQ = RCC\_PLLQ\_DIV2;

RCC\_OscInitStruct.PLL.PLLR = RCC\_PLLR\_DIV2;

**if** (HAL\_RCC\_OscConfig(&RCC\_OscInitStruct) != *HAL\_OK*)

{

Error\_Handler();

}

/\*\* Initializes the CPU, AHB and APB buses clocks

\*/

RCC\_ClkInitStruct.ClockType = RCC\_CLOCKTYPE\_HCLK|RCC\_CLOCKTYPE\_SYSCLK

|RCC\_CLOCKTYPE\_PCLK1|RCC\_CLOCKTYPE\_PCLK2;

RCC\_ClkInitStruct.SYSCLKSource = RCC\_SYSCLKSOURCE\_PLLCLK;

RCC\_ClkInitStruct.AHBCLKDivider = RCC\_SYSCLK\_DIV1;

RCC\_ClkInitStruct.APB1CLKDivider = RCC\_HCLK\_DIV1;

RCC\_ClkInitStruct.APB2CLKDivider = RCC\_HCLK\_DIV1;

**if** (HAL\_RCC\_ClockConfig(&RCC\_ClkInitStruct, FLASH\_LATENCY\_4) != *HAL\_OK*)

{

Error\_Handler();

}

}

/\*\*

\* @brief USART1 Initialization Function

\* @param None

\* @retval None

\*/

**static** **void** **MX\_USART1\_UART\_Init**(**void**)

{

/\* USER CODE BEGIN USART1\_Init 0 \*/

/\* USER CODE END USART1\_Init 0 \*/

/\* USER CODE BEGIN USART1\_Init 1 \*/

/\* USER CODE END USART1\_Init 1 \*/

huart1.Instance = USART1;

huart1.Init.BaudRate = 115200;

huart1.Init.WordLength = UART\_WORDLENGTH\_8B;

huart1.Init.StopBits = UART\_STOPBITS\_1;

huart1.Init.Parity = UART\_PARITY\_NONE;

huart1.Init.Mode = UART\_MODE\_TX\_RX;

huart1.Init.HwFlowCtl = UART\_HWCONTROL\_NONE;

huart1.Init.OverSampling = UART\_OVERSAMPLING\_16;

huart1.Init.OneBitSampling = UART\_ONE\_BIT\_SAMPLE\_DISABLE;

huart1.AdvancedInit.AdvFeatureInit = UART\_ADVFEATURE\_NO\_INIT;

**if** (HAL\_UART\_Init(&huart1) != *HAL\_OK*)

{

Error\_Handler();

}

/\* USER CODE BEGIN USART1\_Init 2 \*/

/\* USER CODE END USART1\_Init 2 \*/

}

/\*\*

\* @brief GPIO Initialization Function

\* @param None

\* @retval None

\*/

**static** **void** **MX\_GPIO\_Init**(**void**)

{

GPIO\_InitTypeDef GPIO\_InitStruct = {0};

/\* GPIO Ports Clock Enable \*/

\_\_HAL\_RCC\_GPIOE\_CLK\_ENABLE();

\_\_HAL\_RCC\_GPIOC\_CLK\_ENABLE();

\_\_HAL\_RCC\_GPIOA\_CLK\_ENABLE();

\_\_HAL\_RCC\_GPIOB\_CLK\_ENABLE();

\_\_HAL\_RCC\_GPIOD\_CLK\_ENABLE();

/\*Configure GPIO pin Output Level \*/

HAL\_GPIO\_WritePin(GPIOE, M24SR64\_Y\_RF\_DISABLE\_Pin|M24SR64\_Y\_GPO\_Pin|ISM43362\_RST\_Pin, *GPIO\_PIN\_RESET*);